Cytec Corp.
Voice: (716) 381-4740
FAX:   (716) 381-0475


Cytec PC-B/16 switch module example for Winows NT.

Installation Procedure:

1)  Copy the file WinRT.sys into the WinNT\System32\Drivers folder.

2)  Have the NT workstation administrator run the program Reg380io.exe.
	
3)  Reboot the workstation.  If the PC-B/16 switch module is 
	not already installed, you may install it at this time. 

4)  Run the example program pc16nt.exe which is located in the 
	Pcb16nt folder.

5)  You may modify the example source code pc16nt.cpp 
	for custom applications.  Make sure you have
	a correct path to the winrtctl.h header file.



Notes:

The application Reg380io.exe will modify the Registry,
so it must be executed by the administrator.
You may view the registry using regedt32.exe.

HKEY_LOCAL_MACHINE
   SYSTEM
       CurrentControlSet
           Services
               WinRT
                  WinRTdev0
                     Parameters
			Section0
			Section1
             
WinRT.sys is a IO Port device driver for ports 380 though 381 HEX.
You may view it under the resources tab (IO PORTS) with winmsd.exe to
verify that it is operating properly.

Contact Cytec if you wish to setup other port addresses.

The WinRT port driver for Windows NT was created using
WinRT development software from Blue Water Systems, Inc.

Blue Water Systems:
(206)-771-3610 (PST)
http://www.bluewatersystems.com 


