LabView Driver for Cytec PCB/24D Driver Module.

Make sure base address is set correctly.
(Board is shipped at 380 Hex, Dip switches 1,2,3,4,5 ON; 6,7,8 OFF)

Run Initialize PC24Drv.vi first when computer is booted.

Run PC24Drv Example.vi to operate the PCB/24D Driver Module.
