Cytec Sample Programs and Port I/O Drivers for MS Win NT.

Make sure the file winRT.sys is in the winNT/system32/drivers folder
	if it is not already there.

Reg310io.exe and Reg380io.exe will modify the NT registry
	to allow port access at 310 Hex and 380 Hex.

These must be run by the NT administrator.
Reboot the machine to load the drivers.

Both programs setup four bytes of address space.

Reg310io.exe -----> ports 310, 311, 312, 313 Hex.
Reg380io.exe -----> ports 380, 381, 382, 383 Hex.

Sample code for pcb/24 driver module is included.
The executable pcb24drv.exe is built @ 380Hex.
